 ***Meyer*** *Truck Mount* 

***Formula Vertical*** *TMR* ***Mixer***

**815 – 1,315 Cubic Foot Capacity Available for Truck Mount Application**

**\*HD Self-Compensating Hydrostatic Drive on F815 / F1015 / F1215**

**Single Drive on Standard Versions / Dual Drive on “Plus” & “Commercial” Units**

**All Feature the *Exclusive Meyer Auger Timing System* for the most precise ration!**

** **

**F1015 LH Side Door w/Slide Tray F1215 Front Door/Flat Belt Conv.**

**Meyer Formula – A Step Ahead of the Rest!**

 ******

***Deluxe In-Cab Touch Screen Display Rear Commodity Door, Integrated back-up***

***Joystick Control & Variable Speed Dial Camera & Bunk Light Pkg - Optional***

***Mixer Load Heights:***

|  |  |  |
| --- | --- | --- |
| Must Add the Distance from the Ground to the Top of the Truck Frame Rails to these Measurements | | |
| **Mixer Model** | **Base Machine (no extension)** | **With Belt Capacity Extensions** |
|  |  |  |
| **F815** | 77” | 83” |
| **F1015** | 90” | 96” |
| **F1215** | 102” | 109” |

See a Meyer Formula Product Brochure for Specifications

***Phone# 1-800-325-9103 meyermfg.com contact us:*** [***sales@meyermfg.com***](mailto:sales@meyermfg.com)